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Technical parameters of 40ft side loader trailer



	Main specification

	Type
	40ft skeleton semi trailer

	Overall dimension (LXWXH) (including the crane)
	14100x2500x4100 mm

	Container twist lock
	8 pcs

	Main beam
	The height of the beam is 500 mm,
upper plate is16mm,
down plate is 18mm,
middle plate is 10mm.

	Side beam
	16U shaped steel or I shaped steel

	Traction pin
	2’ inch or 3.5’ inch

	Land gear
	Standard 28ton

	Axle
	13ton axle x 3 pcs

	Axle brand
	FUWA 

	Suspension type
	mechanical suspension

	Leaf spring
	90mm width, 10mm thickness, 10 pcs

	Tire
	12R22.5 tubeless tyre

	Tire brand
	Triangle

	Tire quantity
	12

	Crane

	Model
	MHQ37A

	Max. Lifting capacity
	37000 kg

	Max. Working range
	4000 mm

	Max. Stabilizer outreach
	3200 mm

	Max. Pressure of Hydraulic
	28 MPa

	Tare weight
	7000kg

	Crane overall dimensions (L x W x H)
	1020 x 2500 x 2490 mm

	Hydraulic system
	Italian CASAPPA hydraulic pump

	
	Netherlandish AMCA hydraulic control valve

	Electric control system
	German NBB telecontroller

	
	12V Voltage

	Chain
	Lgus imported chain, two chains

	Diesel engine
	Japanese Kubota diesel engine

	 Accessories

	Brake
	4 big chamber brake system

	Tool box
	1 unit

	Spare wheel carrier
	1 units

	Side marker lamp
	LED type

	Voltage
	24V

	Receptacle
	7ways (7 wire harness)
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